|  |
| --- |
|  |
| All measurements in mm |  | 0-2-4-6-8 (0 to bow) | **HEADSAIL (JIB)** | | | **MAINSAIL** | | |
|  |  | Mast rake | Mast pos. | Foot chamber | Gap jib boom to mast | Gap at middle  leech to mast | Foot chamber | Gap main boom to CL | Gap 2nd batten to Backstay |
|  | Kit A-Rig (default) GER129 | 1135 | 5 | 25 | 55 | 70 | 30 | 35 | 60 |
|  | Kit A-Rig (light wind) GER95 | 1133 | 7 | 25 | 45 | 50 | 30 | 40 | 47 |
|  | Kit A-Rig (light wind with puffs) GER263 | 1117 | 7 | 33 | 50 | 63 | 30 | 30 | 45 |
|  | Kit A-Rig (big waves) GER95 | 1133 | 7 | 30 | 50 | 75 | 40 | 33 | 68 |
|  | Kit A-Rig (small waves, 2.5 Bft) GER95 | 1127 | 6.5 | 25 | 35 | 50 | 25 | 20 | 40 |
|  | soch sails B-Rig (big waves) GER95 | 970 | 4 | 28 | 50 | 60 | 30 | 23 | 65 |
|  | soch sails B-Rig (small waves) GER95 | 980 | 6 | 32 | 38 | 32 | 30 | 18 | 42 |
|  | soch sails B-Rig (small waves, 2.5 Bft) GER95 | 977 | 7 | 25 | 35 | 55 | 35 | 15 | 40 |
|  | AH-Sails B-Rig (small waves) GER129 | 985 | 7 | 32 | 65 | 77 | 30 | 35 | 50 |
|  | soch sails C-Rig (small waves) GER95 | 850 | 8 | 15 | 40 | 25 | 20 | 15 | 50 |
|  | soch sails C-Rig (choppy waves, 5 Bft) GER95 | 843 | 8 | 30 | 48 | 50 | 35 | 23 | 40 |
|  | soch sails D-Rig (provisional) GER95 | 806 | 8 | 15 | 60 | 65 | 35 | 20 | 45 |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |